Formulation of MT inverse problem

Takuto Minami

Nov. 2, 2021

MT impedance is calculated by Ex and Ey polarization as

Here,

Then

Using these expressions, the form of are derives as

At a given observation site, the following relations holds,

Where denotes polarization. Furtheremore, linear problem for each polarization,

leads to

Using these equations,